{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["钣金","喷漆","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"钣金","index":0,"n_rows":99,"n_cols":6,"rows_kept":99,"merged":[[0,0,0,4],[2,0,21,0],[22,0,42,0],[22,3,22,4],[23,3,23,4],[24,3,24,4],[25,3,25,4],[26,3,26,4],[27,3,27,4],[28,3,28,4],[29,3,29,4],[30,3,30,4],[31,3,31,4],[32,3,32,4],[33,3,33,4],[34,3,34,4],[35,3,35,4],[36,3,36,4],[37,3,37,4],[38,3,38,4],[45,1,51,1],[45,3,51,3],[52,1,55,1],[52,3,55,3],[59,1,61,1],[59,3,61,3],[64,1,68,1],[64,3,68,3],[69,1,73,1],[69,3,73,3],[74,1,80,1],[74,3,75,3],[76,3,77,3],[81,1,83,1],[81,3,83,3],[91,2,91,3],[98,1,98,4]],"flags":["formulas_cached_only"]}
["附件：丰田钣喷项目设备清单"]
["场地","改造方案及补充设备","数量","规格型号","商家、品牌","技术参数及说明"]
["钣金","螺杆式空压机",1,"ITL-30A","泉州力达、英特兰","功率:18KW,最大出气量:3.5M3/MIN/8KG/CM2能够保证6个打磨工位同时工作"]
[]
[null,"气路改造（赠加用气点）",14,"现场施工",null,"共有7个工位，每个工位采用2个可伸缩盘管，是用进口管街头"]
[null,"圆盘式研磨机(配图)",5,"KD8007","广州喜悦","气动"]
[null,"皮带式研磨机(配图)",5,"KD8005","广州喜悦","气动"]
[null,"滚轮式研磨机(配图)",7,500523,"珠海龙神","气动"]
[null,"垫圈焊机（外形修复机）(配图)",6,"FY7000","珠海飞鹰,飞鹰","独特的自动监测电网电压功能,具有焊机温度到达临界时,焊机自动进行冷却状态;功能采用独特高精度时间调整系统;配有多个直拉三角片供直拉钣金时使用;具有多种钣金缩火\\介子\\直拉\\点焊\\压平\\波形线\\螺栓\\OT式拉圈\\三角片等焊接功能;数字化显示;大型拉力器及波纹线焊接;选用世界名牌DELIXI\\OMRON\\PANASONIC继电器,配有气动真空吸盘修复方式"]
[null,"二氧化碳焊机(配图)使用保护气体CO2(20％)+Ar(80％)",5,"FY4220","珠海飞鹰,飞鹰","独特的自动监测电网电压功能,采用HUA有曲向硅钢片100%的铜芯变压器;选用世界知名品牌DELIXI.OMRON.PANASONIC继电器;选用台湾天威档位开关;配有世界知名品牌EMIR焊枪;配有工具盒及焊丝防堵用品数字化显示;多层桥式整流;双轮驱动送丝机构;配加热减压阀;电弧动特性调节;高质量成型焊接,外型美观;空载电压:20-32V;焊接电流:35-250A;暂载率:35%;绝缘等级:F;一元化对应焊接直径:低碳钢实心焊丝0.8,1.0;电压调节级数:6档"]
[null,"气动据",7,"KD8001","广州喜悦","要求可用,配质量高的锯片,最好有进口品牌"]
[null,"打孔器￠5(配图)",7,null,"珠海龙神"]
[null,"手枪式气动钻",7,40227,"珠海龙神"]
[null,"空气枪",7,"国产",null,"长嘴型"]
[null,"钢丝刷",7,"国产",null,"普通"]
[null,"尖嘴钳",7,70112,"上海世达","7寸"]
[null,"工具盒（零件盘）",7,"国产",null,"不锈钢制作"]
[null,"手动剪板机(配图)",1,"国产"]
[null,"钢尺",4,"50CM","上海世达,91403","50CM"]
[null,"车身锉",7,null,"珠海龙神,51023"]
[null,"液压搬运车",2,"1-1.5吨"]
[null,"钣金工具","６套",null,null,"祥见清单"]
["喷漆","气路改造（赠加用气点）",14,"现场施工",null,"共有7个工位，每个工位采用2个可伸缩盘管，是用进口管街头"]
[null,"气路改造（为烤漆房、大梁校正仪供气）","2处","现场施工",null,"与14个工位的同时施工"]
[null,"干磨机（配图及技术参数）",5,"WLTOOL3",null,"每台干磨机配2个打磨头"]
[null,"单作用研磨机",5,"配套",null,"能与干磨机配套使用"]
[null,"￠3双作用研磨机",5,"配套",null,"能与干磨机配套使用"]
[null,"￠7双作用研磨机",5,"配套",null,"能与干磨机配套使用"]
[null,"轨道式研磨机",5,"配套",null,"气动"]
[]
[]
[null,"迷你抛光机",7,"广州喜悦KB-4710",null,"用于局部修补喷漆后抛光"]
[null,"电子秤",1,"WS3XRS-226",null,"最大称重3000G,精度0.1g"]
[null,"吹尘枪",6,"国产",null,"长嘴"]
[null,"标准光源比色灯箱",1,"广州喜悦KB6008"]
[null,"遮蔽纸架",2,"广州喜悦KB-3301",null,"可安装各种规格遮蔽纸"]
[null,"200ml调漆杯",10,"广州喜悦KB-4400",null,"玻璃材质、上下等直径、带刻度"]
[null,"1000ml调漆杯",10,"广州喜悦KB-4401",null,"玻璃材质、上下等直径、带刻度"]
[null,"膜厚测试仪",1,"北京时代TT260",null,"采用磁性和涡流两种测厚方法，可无损测量磁性金属基体上非磁性覆盖层的厚度及飞磁性金属基体上非导电覆盖层的厚度。设五个统计量，存储459个数据；有两种工作方式：直接测量和成组方式；有两种测量方式：连续测量和单次测量；带打印功能，有电源欠压指示边充电边工作。可与电脑通讯，由电脑控制测厚仪工作。配校准标准片"]
[null,"粘度计",1,"深圳NDJ—5",null,"涂-4杯粘度计"]
[null,"秒表",1,"卡西欧HS-30W",null,"10跑道"]
[null,"地网格栅",59,"盐城景中景",null,"1145.5*750*5mm"]
[null,"喷壶",7,"喷除油剂"]
[null,"钣金工具"]
["NO.","工具名称","尺   寸","规格","品牌"]
[1,"十二方套筒扳手","10mm","四方孔9.5mm","世达（SATA）"]
[2,null,"12mm",null,"世达"]
[3,null,"14mm",null,"世达"]
[4,null,"17mm",null,"世达"]
[5,null,"19mm",null,"世达"]
[6,null,"21mm",null,"世达"]
[7,null,"23mm",null,"世达"]
[8,"加长六方套筒扳手","8mm","四方孔9.5mm","世达"]
[9,null,"10mm",null,"世达"]
[10,null,"12mm",null,"世达"]
[11,null,"14mm",null,"世达"]
[12,"棘轮扳手","180mm","安装头9.5mm","世达"]
[13,"滑头手柄","165mm","安装头9.5mm","世达"]
[14,"滑行杆","250mm","安装头12.7mm","世达"]
[15,"延长杆","300mm","四方孔与安装头均9.5mm","世达"]
[16,null,"150mm",null,"世达"]
[17,null,"75mm",null,"世达"]
[18,"万向接头","54mm","四方孔与安装头均9.5mm","世达"]
[19,"变径转换接头",null,"四方孔12.7mm,安装头9.5mm","世达"]
[20,"两用棘轮扳手","10mm","一方扳手、一方棘轮","世达"]
[21,null,"12mm",null,"世达"]
[22,null,"14mm",null,"世达"]
[23,null,"17mm",null,"世达"]
[24,null,"19mm",null,"世达"]
[25,"开口扳手","6×7mm","开口与手柄15°","世达"]
[26,null,"8×10mm",null,"世达"]
[27,null,"10×12mm",null,"世达"]
[28,null,"12×14mm",null,"世达"]
[29,null,"17×19mm",null,"世达"]
[30,"螺丝批","150mm","一字头，通心方杆","世达"]
[31,null,"100mm",null,"世达"]
[32,null,"150mm","十字头，通心方杆","世达"]
[33,null,"100mm",null,"世达"]
[34,null,"短而粗的","一字头","世达"]
[35,null,"短而粗的","十字头","世达"]
[36,null,"细小的","一字头","世达"]
[37,"内六星改锥","T20",null,"世达"]
[38,null,"T25",null,"世达"]
[39,null,"T30",null,"世达"]
[40,"活扳子","330mm","长度257mm","世达"]
[41,"锤子","675gr","长度355mm","世达"]
[42,"中心冲子","125mm",null,"世达"]
[43,"铲刀","180mm","刀刃宽30mm","世达"]
[44,"卷尺","5m",null,"世达"]
[45,"钣金锤套件",null,"7件套","世达"]
[46,"錾子套件",null,null,"世达"]
[47,"手挫","平挫、圆挫、半圆挫、棱形挫、方锉各一",null,"世达"]
[48,"大力钳子组套",null,"7件套","世达"]
[49,"鲤鱼钳",null,null,"世达"]
[50,"尖嘴钳",null,null,"世达"]
[51,"钢丝轮刷",null,"4寸盆形","世达"]
[52,"钢丝轮刷",null,"4寸杆平","世达"]
[]
[null,"说明：上述设备可以报类似配置及要求即可"]

{"sheet":"喷漆","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"merged":[[0,0,0,5],[2,0,18,0]],"flags":["formulas_cached_only"]}

{"sheet":"Sheet2","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}