{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["服务项目"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"服务项目","index":0,"n_rows":11,"n_cols":8,"rows_kept":11,"merged":[[0,0,0,7],[1,0,1,7],[10,0,10,2]]}
["学院配电房电气抽屉开关、直流屏控制柜采购项目-招标采购清单"]
["工程名称：学院配电房电气抽屉开关、直流屏控制柜采购项目                               金额单位：元"]
["序号","项目名称","项目采购需求","单位","采购量","单价","含税合价","备注"]
["一","服务名称",{"$nulls":4},{"$f":"SUM(G5:G6)","v":{"v":0,"d":"0.00"}}]
[1,"CZ3-T5-400低压抽屉开关采购及安装","ABB抽屉开关型号：CZ3-T5-400 ，本次采购的ABB抽屉式开关柜要适用于低压开关柜。","个",2,0,{"$f":"F5*E5","v":0},"   报价时应包含开关价格、运输费、安装费、服务期内的保修服务费、管理费、利润、税金及投标人认为需要的一切费用。"]
[2,"GZDW-60AH/220V直流屏采购及安装","1、2路380V电源输入，直流馈出：6路合闸，6路控制。                                  2.具有温度补偿功能；母线绝缘、支路绝缘、开关量、电池巡检、全自动调压；全自动均浮充转换对蓄电池充电的全自动智能管理；              3.可实现“四遥”功能，提供RS232和RS485接口与上位机通信，达到无人值守；               4.同时满足提供的GZDW-60AH 220V直流屏参数要求；","套",1,0,0," 报价时应包含开关价格、运输费、安装费、服务期内的保修服务费、管理费、利润、税金及投标人认为需要的一切费用。"]
["二","咨询服务费",{"$nulls":4},{"$f":"SUM(G8:G10)","v":4550}]
[1,"方案优化",null,"项",1,2100,{"$f":"F8*E8","v":2100},"为不可竞争费用，不得调整"]
[2,"采购清单及控制价编制",null,"项",1,{"$f":"3000*70%","v":2100},{"$f":"F9*E9","v":2100},"为不可竞争费用，不得调整"]
[3,"项目资料审查",null,"项",1,350,{"$f":"F10*E10","v":350},"为不可竞争费用，不得调整"]
["合     计",{"$nulls":5},0]